{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"merged":[[0,0,0,7],[8,0,8,3],[9,0,9,7]],"flags":["formulas_cached_only"]}
["安徽职业技术学院窗帘制作安装采购项目报价单"]
["序号","名称","技术要求","单位","数量","单价","合价","备注"]
[1,"布料1","米色加密加厚遮光纹面料，幅宽2.8米,其甲醛含量符合环保要求，布四边缝纫卷边，要求美观、大方、高雅，适合办公室环境。","米",512]
[2,"布料2","墨绿或紫红色割绒布，厚度1.6mm，遮光率达到98%，有良好的吸音效果；幅宽2.8米,其甲醛含量符合环保要求，布四边缝纫卷边，要求美观、大方、高雅，适合会议室环境。","米",44]
[3,"布料3","白色多丽印花纱，幅宽2.8米,其甲醛含量符合环保要求，布四边缝纫卷边，要求美观、大方、高雅，适合会议室环境。","米",44]
[4,"轨道（含滑轮、固定卡）","轨（滑）道采用烤漆加厚铝合金窗帘轨道，应是开模而成的型材，规格：高25毫米*宽28毫米；要求材质优良、滑动光滑、噪音小；每窗口轨（滑）道要是一整段型材；滑轮结实、耐用、强度高，抗冲击力强；固定卡强度高，不易变形,固定卡间距不得大于50厘米。","米",300]
[5,"挂勾","铁质镀锌烤漆材料，结实、强度高。","个",2100]
[6,"布带","宽7.5厘米,全棉、白色、结实、耐用。","米",600]
["合计"]
["1、 报价单上的“单价”和“合价”含完成该项目的所有费用\n2、 本报价单不够陈述的，供应商可另附纸进行陈述\n3、 如有不明之处，请与采购人联系，采购人联系电话：0551-64689027（张老师）\n4、 本报价单中的所有采购内容均需提供样品\n5、备注栏由投标单位填写，填写内容为：\n（1）是否与报价单中的名称、型号、技术要求一致，如果一致直接填写一致\n（2）如果与报价单中的名称、型号不一致时，应在满足报价单基本功能的基础上填写所投产品的名称和型号。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}