{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":7,"rows_kept":12,"merged":[[0,0,0,6],[10,1,10,6],[11,0,11,6]],"flags":["formulas_cached_only"]}
["安徽职业技术学院空调安装附属管线报价单"]
["序号","名称","型号","数量","单价","合价","备注"]
[1,"内外机连接小铜管","格力RF280空调室外机对应规格，小铜管直径φ16mm、厚度0.1cm。",140]
[2,"内外机连接大铜管","格力RF280空调室外机对应规格，大铜管直径φ28mm、厚度0.12cm。",140]
[3,"内外机连接电线","空调电线为5*6m2电缆，铜线",150]
[4,"内外机连接信号线","信号线规格：10*1.5m2，铜线",150]
[5,"连接管保温材料","橡塑保温管，直径φ16mm、厚度1.5cm",150]
[6,"连接管保温材料","橡塑保温管，直径φ28mm、厚度1.5cm",150]
[7,"空调包扎带","PVC包扎带，5cm宽，单卷15米以上，黄色","100卷"]
[8,"电源改造","适用格力RF280空调的电源，空调额定功率15kW。5*6m2电线，长度35米，配套空开（60A以上）。需按招标人的要求在指定的位置安装到位，并经验收合格","2套"]
["合计   大写：                                                  小写：","小写：                             大写："]
["1、 报价单上的“单价”和“合价”含完成该项目的所有费用\n2、成交供应商应将成交货物按招标人的要求送至指定位置\n3、 本报价单不够陈述的，供应商可另附纸进行陈述\n4、 如有不明之处，请与采购人联系，采购人联系电话：0551-64680165（张老师）\n5、 本项目采用有效最低价中标，即询价商在满足所有报价单内容的基础上以最低价成交\n6、备注栏由投标单位填写，填写内容为：（1）是否与报价单中的名称、型号一致，如果一致直接填写一致\n（2）如果与报价单中的名称、型号不一致时，应在满足报价单基本功能的基础上填写所投产品的名称和型号。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}